(export (version D)
  (design
    (source "C:/Documents and Settings/Marie/Mes documents/Kicad Projet/Projet Maquette/Maquette.sch")
    (date "17/03/2016 11:13:31")
    (tool "eeschema (2013-07-07 BZR 4022)-stable"))
  (components
    (comp (ref U1)
      (value PIC16F690)
      (libsource (lib microchip) (part PIC16F690))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DBBE))
    (comp (ref R6)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC1D))
    (comp (ref R3)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC36))
    (comp (ref R2)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC45))
    (comp (ref R12)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC54))
    (comp (ref R11)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC63))
    (comp (ref R8)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC72))
    (comp (ref R1)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC81))
    (comp (ref R4)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC90))
    (comp (ref R5)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DC9F))
    (comp (ref R10)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DCAE))
    (comp (ref R9)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DCBD))
    (comp (ref R7)
      (value 5k6)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DCCC))
    (comp (ref Q1)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DEA3))
    (comp (ref Q3)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DEB2))
    (comp (ref Q5)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DEC1))
    (comp (ref Q2)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DED0))
    (comp (ref Q4)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DEDF))
    (comp (ref Q6)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DEEE))
    (comp (ref Q7)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DEFD))
    (comp (ref Q9)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DF0C))
    (comp (ref Q11)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DF1B))
    (comp (ref Q12)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DF2A))
    (comp (ref Q8)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DF39))
    (comp (ref Q10)
      (value BC550)
      (footprint TO92)
      (libsource (lib transistors) (part BC550))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7DF57))
    (comp (ref P10)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E024))
    (comp (ref P11)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E033))
    (comp (ref P14)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E042))
    (comp (ref P13)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E051))
    (comp (ref P12)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E060))
    (comp (ref P9)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E06F))
    (comp (ref P5)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E07E))
    (comp (ref P4)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E08D))
    (comp (ref P3)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E09C))
    (comp (ref P1)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E0AB))
    (comp (ref P2)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E0BA))
    (comp (ref P6)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E0C9))
    (comp (ref P7)
      (value CONN_5)
      (libsource (lib conn) (part CONN_5))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E58B))
    (comp (ref P8)
      (value CONN_2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E7E816)))
  (libparts
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib transistors) (part BC547)
      (description "BC547, 45V Vce, 0.1A Ic, NPN, Small Signal Transistor,TO-92")
      (docs http://www.fairchildsemi.com/ds/BC/BC547.pdf)
      (footprints
        (fp TO92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC547)
        (field (name Footprint) TO92)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name C) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_5)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_5))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))))
    (libpart (lib microchip) (part PIC16F690)
      (fields
        (field (name Reference) U)
        (field (name Value) PIC16F690))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name RA5/T1CKI/OSC1/CLKIN) (type BiDi))
        (pin (num 3) (name RA4/AN3/T1G/OSC2/CLKOUT) (type BiDi))
        (pin (num 4) (name RA3/MCLR/VPP) (type BiDi))
        (pin (num 5) (name RC5/CCP1/P1A) (type BiDi))
        (pin (num 6) (name RC4/C2OUT/P1B) (type BiDi))
        (pin (num 7) (name RC3/AN7/C12IN3-/P1C) (type BiDi))
        (pin (num 8) (name RC6/AN8/SS) (type BiDi))
        (pin (num 9) (name RC7/AN9/SDO) (type BiDi))
        (pin (num 10) (name RB7/TX/CK) (type BiDi))
        (pin (num 11) (name RB6/SCK/SCL) (type BiDi))
        (pin (num 12) (name RB5/AN11/RX/DT) (type BiDi))
        (pin (num 13) (name RB4/AN10/SDI/SDA) (type BiDi))
        (pin (num 14) (name RC2/AN6/C12IN2-/P1D) (type BiDi))
        (pin (num 15) (name RC1/AN5/C12IN1-) (type BiDi))
        (pin (num 16) (name RC0/AN4/C2IN+) (type BiDi))
        (pin (num 17) (name RA2/AN2/T0CKI/INT/C1OUT) (type BiDi))
        (pin (num 18) (name RA1/AN1/C12IN0-/VREF/ICSPCLK) (type BiDi))
        (pin (num 19) (name RA0/AN0/C1IN+/ICSPDAT/ULPWU) (type BiDi))
        (pin (num 20) (name VSS) (type power_in)))))
  (libraries
    (library (logical transistors)
      (uri "C:\\Program Files\\KiCad\\share\\library\\transistors.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\library\\device.lib"))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\library\\conn.lib"))
    (library (logical microchip)
      (uri "C:\\Program Files\\KiCad\\share\\library\\microchip.lib")))
  (nets
    (net (code 1) (name "")
      (node (ref P1) (pin 1))
      (node (ref Q1) (pin 3)))
    (net (code 2) (name "")
      (node (ref Q6) (pin 3))
      (node (ref P5) (pin 1)))
    (net (code 3) (name "")
      (node (ref P4) (pin 1))
      (node (ref Q4) (pin 3)))
    (net (code 4) (name "")
      (node (ref P3) (pin 1))
      (node (ref Q2) (pin 3)))
    (net (code 5) (name "")
      (node (ref Q3) (pin 3))
      (node (ref P2) (pin 1)))
    (net (code 6) (name "")
      (node (ref Q5) (pin 3))
      (node (ref P6) (pin 1)))
    (net (code 7) (name "")
      (node (ref R2) (pin 1))
      (node (ref Q4) (pin 2)))
    (net (code 8) (name "")
      (node (ref Q10) (pin 1))
      (node (ref P8) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref Q11) (pin 1))
      (node (ref Q12) (pin 1))
      (node (ref Q5) (pin 1))
      (node (ref Q8) (pin 1))
      (node (ref U1) (pin 20))
      (node (ref Q9) (pin 1))
      (node (ref Q7) (pin 1))
      (node (ref Q3) (pin 1))
      (node (ref Q6) (pin 1))
      (node (ref Q4) (pin 1))
      (node (ref Q2) (pin 1)))
    (net (code 9) (name "")
      (node (ref Q8) (pin 3))
      (node (ref P9) (pin 1)))
    (net (code 10) (name "")
      (node (ref Q10) (pin 3))
      (node (ref P12) (pin 1)))
    (net (code 11) (name "")
      (node (ref R1) (pin 1))
      (node (ref Q6) (pin 2)))
    (net (code 12) (name "")
      (node (ref Q2) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 13) (name "")
      (node (ref R4) (pin 1))
      (node (ref Q1) (pin 2)))
    (net (code 14) (name "")
      (node (ref Q3) (pin 2))
      (node (ref R5) (pin 1)))
    (net (code 15) (name "")
      (node (ref R6) (pin 1))
      (node (ref Q5) (pin 2)))
    (net (code 16) (name "")
      (node (ref P7) (pin 1))
      (node (ref U1) (pin 2)))
    (net (code 17) (name "")
      (node (ref U1) (pin 1))
      (node (ref P8) (pin 2)))
    (net (code 18) (name "")
      (node (ref U1) (pin 18))
      (node (ref P7) (pin 4)))
    (net (code 19) (name "")
      (node (ref P7) (pin 2))
      (node (ref U1) (pin 3)))
    (net (code 20) (name "")
      (node (ref U1) (pin 4))
      (node (ref P7) (pin 3)))
    (net (code 21) (name "")
      (node (ref P7) (pin 5))
      (node (ref U1) (pin 17)))
    (net (code 22) (name "")
      (node (ref Q7) (pin 3))
      (node (ref P10) (pin 1)))
    (net (code 23) (name "")
      (node (ref Q7) (pin 2))
      (node (ref R7) (pin 2)))
    (net (code 24) (name "")
      (node (ref U1) (pin 9))
      (node (ref R5) (pin 2)))
    (net (code 25) (name "")
      (node (ref R7) (pin 1))
      (node (ref U1) (pin 16)))
    (net (code 26) (name "")
      (node (ref U1) (pin 14))
      (node (ref R9) (pin 1)))
    (net (code 27) (name "")
      (node (ref U1) (pin 13))
      (node (ref R10) (pin 1)))
    (net (code 28) (name "")
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 8)))
    (net (code 29) (name "")
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 5)))
    (net (code 30) (name "")
      (node (ref R8) (pin 2))
      (node (ref Q9) (pin 2)))
    (net (code 31) (name "")
      (node (ref U1) (pin 19)))
    (net (code 32) (name "")
      (node (ref R6) (pin 2))
      (node (ref U1) (pin 10)))
    (net (code 33) (name "")
      (node (ref U1) (pin 7))
      (node (ref R3) (pin 2)))
    (net (code 34) (name "")
      (node (ref U1) (pin 6))
      (node (ref R2) (pin 2)))
    (net (code 35) (name "")
      (node (ref R12) (pin 1))
      (node (ref U1) (pin 11)))
    (net (code 36) (name "")
      (node (ref U1) (pin 12))
      (node (ref R11) (pin 1)))
    (net (code 37) (name "")
      (node (ref R11) (pin 2))
      (node (ref Q10) (pin 2)))
    (net (code 38) (name "")
      (node (ref U1) (pin 15))
      (node (ref R8) (pin 1)))
    (net (code 39) (name "")
      (node (ref Q11) (pin 2))
      (node (ref R9) (pin 2)))
    (net (code 40) (name "")
      (node (ref R10) (pin 2))
      (node (ref Q12) (pin 2)))
    (net (code 41) (name "")
      (node (ref Q8) (pin 2))
      (node (ref R12) (pin 2)))
    (net (code 42) (name "")
      (node (ref Q9) (pin 3))
      (node (ref P11) (pin 1)))
    (net (code 43) (name "")
      (node (ref Q11) (pin 3))
      (node (ref P14) (pin 1)))
    (net (code 44) (name "")
      (node (ref P13) (pin 1))
      (node (ref Q12) (pin 3)))))